1.CHECK PUSH-BUTTON IGNITION SWITCH OPERATION Check push-button ignition switch operation. Refer to System Description. Is the inspection result normal? YES>>GO TO 2.
NO>>Refer to Description.
2.CHECK PUSH-BUTTON IGNITION SWITCH INDICATOR
Check push-button ignition switch indicator.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 3.
NO>>Repair or replace the malfunctioning parts.
3.CONFIRM THE OPERATION
Confirm the operation again.
Is the result normal?
YES>>Check intermittent incident. Refer to Intermittent Incident.
NO>>GO TO 1.