| Wiring Diagram |  |  |
| 1 | General Outline |  |
| The following are the four main functions of the electronic wiring diagram: |
| - Circuit Diagram |
| - Harness Layout |
| - Power Source |
| - Connector Search |
| In addition, connector detail and connected circuit information can be viewed in split window mode. |
| 2 | Preinclination |  |
| For Internet Explorer 7.0, it have to change the following setting on client PC at first time of using the electronic wiring diagrams. |
| 2-1 | Turn off pop-up broker. |

| 2-2 | Allow websites to open windows without address or status bars. |
| 2-3 | Allow script-initiated windows without size or position constrains. |

| 3 | Window Image |  |
| 3-1 | Initial screen |
| The initial screen of the Electronic Wiring Diagram displays as follows: |

| No. | Item | Description |
| 1 | [Circuit Diagram] Button | To find the circuit diagram from the section. |
| 2 | [Harness Layout] Button | To find the connector or harness routing from the location. |
| 3 | [Power Source] Button | To find the power source from the fuse or fusible link. |
| 4 | [Connector Search] Button | To find connector from the connector name or number. |
| 3-2 | Viewing options |

| No. | Item | Description |
| ① | Connector List | Displays connector names and numbers that are shown in the circuit diagram or harness layout. Clicking the connector changes the color of the corresponding connector in the main screen. In addition, the connector detail is displayed. |
| ② | Connector Detail | Displays details of the selected connector. |
| ②-1 | Connector information column | Displays connector number, connector name and connector color (connector type). Connector type indicates connector color as: RS04FG-GY -> G: Green |
| ②-2 | Connector view change button | Alternates between harness side and terminal side connector views. |
| ②-3 | Connector view icon | Shows the current connector view selected (terminal side or harness side). |
| ②-4 | Connector shape | Displays the terminal arrangement of the connector. |
| ②-5 | Terminal information | Displays terminal number, wire color, and signal name. Terminals not available are indicated as "-". Clicking the terminal number in light blue displays all connections to that terminal. |
| ②-6 | Hyper link to related information | Hyper links to related harness information are shown. Clicking the hyper link opens the corresponding harness layout or circuit diagram. |
| ②-7 | Zoom button | Enlarges the connector shape. |
| ②-8 | Standard view button | Connector shape returns to the original size. |
| 3 | Layer indication | Shows the section, sub-section and title for the main screen. From here, it is possible to select the section or sub-section without returning to the initial screen. |
| 4 | Frame size adjustment button | Frame size of the screen can be switched by this button. Click the button to switch between split window view and full screen. (Note: Screen size can also be adjusted by sliding the frame.) |
| 5 | Main screen | Displays the circuit diagram, harness layout, power source or connector search screen. |
| ⑤-1 | Zoom out button | Reduces the main screen display size. |
| ⑤-2 | Standard view button | Returns the main screen display size to the original size. |
| ⑤-3 | Zoom in button | Enlarges the main display. |
| ⑤-4 | Full-page view button | Sizes the main display to full-page view. |
| ⑤-5 | Print button | Displays PDF pages of the screen display to allow printing. |
| ⑤-6 | Initial screen button | Returns to the initial screen of the Electronic Wiring Diagram. |
| ⑤-7 | Display area movement | Click and hold the left mouse button on an open area to move the main screen display area. |
| 4 | Function Description |  |
| 4-2 | Circuit Diagram |
| 4-2-1 | Circuit Diagram Selection |
| After selecting Circuit Diagram from the initial screen of the Electronic Wiring Diagram, |
| click the appropriate title to open the initial screen of the selected schematic. |

| 4-2-2 | Circuit Diagram |

| 4-3 | Harness Layout |
| 4-3-1 | Harness Layout Selection |
| Select appropriate harness in SECTION or OUTLINE to show the harness layout screen. |

| 4-3-2 | Harness Layout |

| 4-4 | Power Source |  |
| 4-4-1 | Power Source Diagram Selection |
| Select appropriate power source by SECTION -> SUB-SECTION -> TITLE. |
| For the entire schematic of BATTERY, ACCESSORY or IGNITION, click the first title (BATTERY POWER SUPPLY). |
| The downstream detail power source diagrams of the BATTERY, ACCESSORY or IGNITION are aligned from the 2nd title. |
| Click the button at the bottom of the page to open the initial screen of the Electronic Wiring Diagram. |

| 4-4-2 | Power Supply Routing Circuit |

| 4-4-3 | Power Supply Downstream Detail |

| 4-4-4 | Fuse Block and IPDM Layout |

| 4-5 | Connector Search |
| 4-5-1 | Connector Search |
| Information for a particular connector can be found using the connector search function. |

| Back To Help Top |  |  | Go To Next Topic |  |  |