■ CAUTION ■

- Disconnect the battery negative terminal or remove the fuse.
- Never touch the glass of bulb directly by hand. Keep grease and other oily matters away from it.
- Never touch bulb by hand while it is lit or right after being turned off.
- Never leave bulb out of lamp reflector for a long time because dust, moisture smoke, etc. may affect the performance of lamp. When replacing bulb, be sure to replace it with new one.

FRONT SIDE MARKER LAMP BULB

1.Remove the front side marker lamp. Refer to Exploded View.

2.Turn the bulb socket (1) counterclockwise and unlock it.

3.Remove the bulb (2) from the socket.