DTC DETECTION LOGIC

DTC | Display Item | Malfunction detected condition | Possible causes
C1D03 | ST ANGLE SPEED SIG |

- A malfunction is detected in the steering angle speed sensor signal output from the steering angle sensor to CAN communication.
- No transmission of the steering angle speed signal from the steering angle sensor.

- Harness or connector (CAN communication line)
- Steering angle sensor
- E-SUS control unit

DTC REPRODUCTION PROCEDURE
1.DTC REPRODUCTION PROCEDURE
With CONSULT-III

1. Turn the ignition switch OFF to ON.
2. Perform “E-SUS” self-diagnosis.

Is DTC “C1D03” detected?
YES>>Proceed to diagnosis procedure. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END