1. | Companion flange | 2. | Front oil seal | 3. | Transmission assembly
| : Apply anti-corrosion oil. |  |  |  |
| : Check that the grease is applied to the lip and all inner walls of front oil seal. Apply multi-purpose grease or equivalent if the grease is not applied. Refer to Removal and Installation (GT-R certified NISSAN dealer). ■ CAUTION ■ Never use including extreme pressure additives.
Refer to Components in GI section for the symbols other than above.