■ CAUTION ■

- Never spill or splash brake fluid on painted surfaces. Brake fluid may seriously damage paint. Wipe it out immediately and wash with water if it gets on a painted surface.
- Turn the ignition switch OFF and disconnect the ABS actuator and electric unit (control unit) connector or the battery negative terminal before performing work.
- Wrap the flare nut wrench with waste cloth to protect the caliper from damage.
- If the brake fluid adheres to the caliper or disc rotor, quickly wipe it out.

1.Remove tires. Refer to Exploded View.

2.Connect a vinyl tube to the bleeder valve.

3.Depress the brake pedal and loosen the bleeder valve to gradually discharge brake fluid.