DISASSEMBLY

1.Remove intake manifold collector. Refer to Exploded View.
■ CAUTION ■
Mark the parts with paint in advance of the reinstallation to prevent misalignment between the intake manifold collector and intake manifold.

2.Remove fuel injector and fuel tube assembly. Refer to Exploded View.

3.Remove intake manifold. Refer to Exploded View.

4.Remove ignition coil, spark plug and rocker cover. Refer to Exploded View.

5.Remove front timing chain case. Refer to Exploded View (GT-R certified NISSAN dealer).

6.Remove oil pan (lower and upper). Refer to Exploded View (GT-R certified NISSAN dealer).

7.Remove rear timing chain case. Refer to Exploded View (GT-R certified NISSAN dealer).

8.Remove exhaust manifold and turbocharger assembly. Refer to Exploded View.

9.Remove camshaft. Refer to Exploded View (GT-R certified NISSAN dealer).

10.Remove cylinder head. Refer to Exploded View (GT-R certified NISSAN dealer).

ASSEMBLY
Assembly in the reverse order of disassembly.