■ CAUTION ■

- When removing/installing the rear final drive, note the following and remove/install the transmission assembly as a set. Refer to Exploded View (GT-R certified NISSAN dealer).

- Install (A) with the paint mark (Y) on the air breather hose (1) facing upward from the vehicle. Be sure to insert air breather hose to air breather tube until hose end reaches the tube bend R portion.
- Be sure to install the air breather hose clip (2) in (B) of the bracket (3).
- Install (C) with the paint mark (Y) facing downward from the vehicle. Be sure to insert it until it contacts a tube end.
- Make sure there are no pinched or restricted areas on the breather hose caused by bending or winding when installing it.