Drive type | AWD
Engine | VR38DETT
Transmission | GR6Z30A
Propeller shaft model | 3F56A-DOJ75
Number of joints | 3
Type of journal bearings (Non-disassembly type) | 1st joint | CVJ type
2nd joint | Cardan type
3rd joint | Cardan type
Coupling method with transmission | Flange type
Coupling method with front final drive | Flange type
Shaft length | 1st (Spider to spider) | 855 mm (33.66 in)
2nd (Spider to spider) | 750 mm (29.53 in)
Shaft outer diameter | 1st | 50.8 mm (2.000 in)
2nd | 42.7 mm (1.681 in)