For this vehicle, the body structural tolerances is decreased. Therefore, if the dimension is outside the standard, not only the intrinsic performance for this vehicle is degraded, but also malfunctions such as the uneven tire wear or wind noise may occur.
To make high accurate body repair effectively and keep good repair quality, NISSAN recommend to use CELETTE® advanced collision repair equipment for this vehicle body repair. CELETTE® equipment is approved by NISSAN for this vehicle body structure repair.
See following recommended equipment.

Recommended equipment: | CELETTE® jig bench
| CELETTE® MZ + System

- Universal Piston: 25000.000

- Tops (Jig Heads for Underbody): 2506.500

- Tops (Jig Heads for Bodyside): 2506.800

| Need ″Overhead gantry supports (9113.63) to use ″Jig Heads for Bodyside″