DTC DETECTION LOGIC

DTC | Display item | Malfunction detected condition | Possible cause
C1193 | VALVE SET | Calibration of valve is not complete. |

- ABS actuator and electric unit (control unit)
- Valve calibration is not yet performed.

DTC CONFIRMATION PROCEDURE
1.DTC REPRODUCTION PROCEDURE

1. Turn the ignition switch ON.
2. Perform pressure sensor calibration. Refer to Description (GT-R certified NISSAN dealer).
3. Perform valve calibration. Refer to Description (GT-R certified NISSAN dealer).
4. Perform self-diagnosis for “ABS” with CONSULT-III.

Is DTC “C1193” detected?
YES>>Proceed to diagnosis procedure. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END