1.CHECK METER CONTROL SWITCH SIGNAL CIRCUIT Perform the meter control switch signal circuit inspection. Refer to Diagnosis Procedure. Is the inspection result normal? YES>>GO TO 2. NO>>Repair the harnesses or connectors.
2.CHECK METER CONTROL SWITCH
Perform the unit inspection of meter control switch. Refer to Component Inspection.
Is the inspection result normal?
YES>>Replace the combination meter.
NO>>Replace the meter control switch.