1.PERFORM ABS ACTUATOR AND ELECTRIC UNIT (CONTROL UNIT) SELF-DIAGNOSIS With CONSULT-III Perform self-diagnosis of the ABS actuator and electric unit (control unit). Refer to CONSULT-III Function (GT-R certified NISSAN dealer). Is DTC detected? YES>>Check malfunctioning circuit.
NO>>GO TO 2.
2.PERFORM THE SELF-DIAGNOSIS
With CONSULT-III
Perform self-diagnosis of the low tire pressure warning control unit.
Is DTC “C1729” detected?
YES>>Replace the low tire pressure warning control unit.
NO>>GO TO 3.
3.CHECK INFORMATION
With CONSULT-III
Use CONSULT-III “DATA MONITOR” to check the input/output values. Refer to Reference Value (GT-R certified NISSAN dealer).
Is the inspection result normal?
YES>>Check pin terminal and connection of each harness connector for malfunctioning conditions.
NO>>Replace the low tire pressure warning control unit.