- The line pressure sensor is installed on the actuator control module and detects the line pressure.
- The line pressure sensor converts the line pressure into output voltage and transmits the signal to TCM. TCM uses this signal in calculations for control switching or other functions.
- The line pressure sensor output voltage varies depending on the pressure variations. The voltage increases as the pressure increases.