1.CHECK DTC WITH TRANSMISSION With CONSULT-III

1. Turn ignition switch ON.
2. Check “Self Diagnostic Result” of “TRANSMISSION”.

Is the inspection result normal?
YES>>GO TO 2.
NO>>Check DTC detected item. Refer to DTC Index.
2.DETECT MALFUNCTIONING ITEM
Check the following harness connector pin terminals for any malfunctions on the connections, harness sheath or other areas. Refer to Intermittent Incident

- Control device harness connector
- Paddle shifter (shift-up switch) harness connector
- Paddle shifter (shift-down switch) harness connector
- TCM harness connector
- Transmission harness connector
- Park position switch harness connector
- Combination meter harness connector

Is the inspection result normal?
YES>>Replace the combination meter. Refer to Exploded View.
NO>>Repair or replace damaged parts.