■ CAUTION ■ Thoroughly read and understand the vehicle specification. Incorrect settings may result in abnormal control of ECU.

MANUAL SETTING ITEM | NOTE
Items | Setting value
AUTO LIGHT | WITH ⇔ WITHOUT | —
DTRL | WITH ⇔ WITHOUT |

- WITH: With daytime running light system
- WITHOUT: Without daytime running light system

⇔: Items which confirm vehicle specifications

AUTO SETTING ITEM | NOTE
Items | Setting value
ROOF FUNCTION | W/O REQ SW | —
WELCOME LIGHT SELECT | WITHOUT | —
H/L BULB | DEFAULT | —
FR FOG LAMP | WITH | Even on a vehicle without front fog lamp. It displays “WITH”.
RR FOG LAMP | WITH | Even on a vehicle without rear fog lamp. It displays “WITH”.
HANDLE | LHD | —
DI LMP VARIAT | MODE3 | —
LIGHT RECOG | MODE4 | —
TRANSMISSION | TRANSMISSION | —
REVERSE BUZZER | WITH | —
RAIN SENSOR | WITHOUT | —
HAZARD SW TYPE | MODE2 | —
BCM AC CONTROL | MODE1 | —
TPMS | TPMS SBF | —
RR WIPER GND | MODE1 | —
DROP WIP FUNCTION | WITHOUT | —