1. | Gear carrier | 2. | Side oil seal | 3. | Side flange
4. | Filler plug | 5. | Gasket | 6. | Drain plug
7. | Side bearing adjusting shim | 8. | Side bearing | 9. | Drive gear
10. | Differential case assembly | 11. | O‐ring | 12. | Side cover
A. | Oil seal lip | B. | Screw hole | C. | Comply with the assembly procedure when tightening. Refer to Assembly (GT-R certified NISSAN dealer).
D. | Use an installed part, because it never be replaced alone. |  |  |  |
: Apply gear oil.
: Apply anti-corrosion oil.
: Apply Genuine High Strength Thread Locking Sealant or equivalent. Refer to Recommended Chemical Products and Sealants.
Refer to Components for symbols not described above.