- The Intelligent Key system is a system that makes it possible to lock and unlock the door locks (door lock/unlock function) by carrying the Intelligent Key, which operates based on the results of electronic ID verification using two-way communications between the Intelligent Key and the vehicle (BCM).
  ■ CAUTION ■
  The driver should always carry the Intelligent Key
- The settings for each function can be changed with the CONSULT-III.
- If an Intelligent Key is lost, a new Intelligent Key can be registered. A maximum of 4 Intelligent Keys can be registered.
- It is possible to perform a diagnosis on the system and register an Intelligent Key with CONSULT-III.

Function | Description | Refer
Door lock function | Lock/unlock can be performed by pressing the request switch. | System Description
Remote keyless entry function | Lock/unlock can be performed by pressing the remote controller button of the Intelligent Key. | System Description
Trunk open function | The trunk lid can be opened by carrying the Intelligent Key and pressing the trunk lid opener request switch. | System Description
Key reminder function | The key reminder buzzer sounds a warning if the door is locked with the key left inside the vehicle. | System Description
Warning function | If an action that does not meet the operating condition of the Intelligent Key system is taken, the buzzer sounds to inform the driver. | System Description
Engine start function | The engine be turned on while carrying the Intelligent Key. | System Description