REMOVAL

1.Disconnect accelerator pedal position sensor harness connector.

2.Remove accelerator pedal assembly.
■ CAUTION ■

- Never disassemble accelerator lever. Never remove accelerator pedal position sensor from accelerator lever.
- Never impact or drop accelerator pedal assembly during handling.
- Be careful to keep accelerator lever away from water.

INSTALLATION
Install in the reverse order of removal.