Bilstein DampTronic system

- When detecting any malfunction in each component of the system, it enters the fail-safe status (the Bilstein DampTronic system control is deactivated).
- At the same time when the system enters the control stop status, it becomes the equivalent status to R mode (fixed damping status).
- Even if the set-up switch (suspension) is operated in the fail-safe status, no lamp illuminates in R mode or COMFORT mode.