Bank 1 side

1. | Exhaust manifold cover | 2. | Insulator (upper) | 3. | Clamp
4. | Fresh air hose | 5. | Fresh air tube | 6. | Gasket
7. | Recirculation hose | 8. | Air inlet pipe | 9. | Gasket
10. | Vacuum hose | 11. | Exhaust manifold and turbocharger assembly | 12. | Oil return hose
13. | Clamp | 14. | Insulator (lower) | 15. | Oil return tube
16. | Gasket | 17. | Gasket | 18. | Water inlet tube
19. | Clamp | 20. | Water hose | 21. | Clamp
22. | Water hose | 23. | Water outlet tube | 24. | Gasket
25. | Bracket |  |  |  |
A. | To rocker cover (bank 1) | B. | To recirculation valve (bank 1) | C. | To air cleaner (bank 1)
D. | To turbocharger boost control solenoid valve | E. | To charge air cooler | F. | To oil filter bracket
G. | To cylinder block | H. | To three way catalyst (bank 1) | I. | To heater pipe
J. | To air cut solenoid valve (bank 2) |  |  |  |
Refer to Components for symbols in the figure.

Bank 2 side

1. | Gasket | 2. | Oil temperature sensor | 3. | Oil feed adapter
4. | Oil feed tube (bank 1) | 5. | Gasket | 6. | Clamp
7. | Fresh air hose | 8. | Fresh air tube | 9. | Gasket
10. | Recirculation hose | 11. | Air inlet pipe | 12. | Clamp
13. | Vacuum hose | 14. | Vacuum hose | 15. | Vacuum hose
16. | Turbocharger boost control solenoid valve | 17. | Vacuum hose | 18. | Vacuum hose
19. | 3- WAY connector | 20. | Gasket | 21. | Clamp
22. | Oil return hose | 23. | Insulator (lower) | 24. | Oil return tube
25. | Gasket | 26. | Gasket | 27. | Water inlet tube
28. | Water outlet tube | 29. | Clip | 30. | Clamp
31. | Water hose | 32. | Insulator (upper) | 33. | Exhaust manifold cover
34. | Oil feed tube | 35. | Bracket | 36. | Gasket
37. | Exhaust manifold and turbocharger assembly |  |  |  |
A. | To exhaust manifold and turbocharger assembly (bank 1) | B. | To cylinder block | C. | To rocker cover (bank 2)
D. | To recirculation valve (bank 2) | E. | To air cleaner (bank 2) | F. | To exhaust manifold and turbocharger assembly (bank 1)
G. | To oil pan (upper) | H. | To charge air cooler | I. | To cylinder block
J. | To three way catalyst (bank 2) | K. | To heater pipe |  |
Refer to Components for symbols in the figure.