1.CHECK TRUNK LID OPENER CANCEL SWITCH Check trunk lid opener cancel switch position. Does trunk lid opener cancel switch turn ON (CANCEL)? YES>>Turn off trunk lid opener cancel switch. NO>>GO TO 2.
2.CHECK FUNCTION
Check (“TR/BD OPEN SW”) in “Data Monitor” mode using CONSULT-III.

Monitor item | Condition | Status
TR/BD OPEN SW | Trunk lid opener switch | Pressed | ON
Released | OFF

Is the inspection result normal?
YES>>Trunk lid opener switch is OK.
NO>>Refer to Diagnosis Procedure.