REMOVAL

1. | Starter motor protector | 2. | “B” terminal harness | 3. | Starter motor“B” terminal nut
4. | “S” connector | 5. | Starter motor | 6. | Starter motor mounting bolt
: Engine front
Refer to Components for symbols in the figure.

DISASSEMBLY
Type: M000T22771

1. | Magnetic switch assembly | 2. | Adjusting plate | 3. | Metal FR
4. | Gear case assembly | 5. | Stopper ring | 6. | Stopper
7. | Pinion assembly | 8. | Yoke assembly | 9. | Armature assembly
10. | Brush holder assembly | 11. | Metal RR | 12. | Rear cover assembly
13. | Planetary gear | 14. | Packing | 15. | Plate
16. | Shift lever set | 17. | Internal gear | 18. | Packing
19. | Gear shaft |  |  |  |
: High-temperature grease point
Refer to Components for symbols not described on the above.