1.ADJUSTMENT OF STEERING ANGLE SENSOR NEUTRAL POSITION

- After replacing an ABS actuator and electric unit (control unit), be sure to perform the following procedure.

- Steering angle sensor adjustment: Refer to Description (GT-R certified NISSAN dealer).
- Decel G sensor calibration: Refer to Description (GT-R certified NISSAN dealer).
- Pressure sensor calibration: Refer to Description (GT-R certified NISSAN dealer).
- Valve calibration: Refer to Description (GT-R certified NISSAN dealer).

- After replacing a steering angle sensor, be sure to perform the following procedure.

- Steering angle sensor adjustment: Refer to Description (GT-R certified NISSAN dealer).

>>END