1. | BCM M118, M119, M121, M122, M123 | 2. | IPDM E/R E5, E6, F7 | 3. | Combination meter M53
4. | TCM B45 | 5. | Push button ignition switch M131 | 6. | Stop lamp switch E110
7. | Combination meter (Key warning lamp) M53 |  |  |  |
A. | Behind the instrument lower panel (RH) | B. | Engine room dash panel (RH) | C. | View with trunk front finisher removed
D. | View with instrument lower panel (driver) removed | E. | Located on the conbination meter |  |