1.CHECK DTC WITH “ABS ACTUATOR AND ELECTRIC UNIT (CONTROL UNIT)” Check “Self diagnostic result” with CONSULT-III. Refer to DTC No. Index. Is the inspection result normal? YES>>GO TO 2. NO>>Repair or replace the malfunctioning parts.
2.CHECK DTC WITH “COMBINATION METER”
Check “Self diagnostic result” with CONSULT-III. Refer to DTC Index.
Is the inspection result normal?
YES>>GO TO 3.
NO>>Repair or replace the malfunctioning parts.
3.CHECK INTERMITTENT INCIDENT
Refer to Intermittent Incident.
>>INSPECTION END