In addition to the regular maintenance recommended by NISSAN, the GT-R requires the following Inspections;

- Measurement and adjustment of wheel Alignment NOTE (1)
- Transmission settings NOTE (2)
- Engine setting (balancing of air flow for bank 1 and bank 2) NOTE (3)

These inspections are required at the following intervals: 1,000 miles, 12 months, 24 months and 36 months.
These inspections will be performed free of charge only at a GT-R certified NISSAN dealer. See the NISSAN GT-R Warranty Information Booklet for details.
After the four free inspections, these items are included in the regular scheduled maintenance.
*Repairs and adjustments involving part replacement, etc. determined to be necessary as a result of these inspections must be performed at the customer's expense.

Inspection item | Inspection timing (Miles/Months) | Remarks
1,000 | 12M | 24M | 36M
Measurement and adjustment of wheel alignment (Unladen*1) | X | X | X | X | Front | Wheel Alignment*2
Rear | Wheel Alignment
Transmission settings | X | X | X | X | –
Engine settings (balancing of air flow for bank 1 and bank 2) | X | X | X | X | –
X: Applicable
*1: Fuel full
*2: Kingpin inclination data are just reference values.
NOTE：
(1) This vehicle is equipped with a high performance suspension. As the suspension components “break-in”, the vehicle's wheel alignment needs to be measured and adjusted by a GT-R certified NISSAN dealer at the recommended intervals.When manufactured, the GT-R front and rear wheel alignment is set to Performance driving settings. The front end alignment can be adjusted to either Performance or Normal/Street settings. Please consult with your GT-R certified NISSAN dealer to determine the optimum setting for the GT-R. Refer to Inspection and Inspection.
(2) The design of the clutch and transmission requires inspection and adjustment of the clutch and shift forks by a GT-R certified NISSAN dealer at the recommended intervals. If the vehicle is regularly driven in performance driving conditions, more frequent adjustments may be necessary to help maximize vehicle performance. Refer to Description (GT-R certified NISSAN dealer).
(3) Each cylinder bank of this engine operates independently due to the vehicle's twin turbocharger design. Each side of the engine must operate at the same level of performance. The air flow of each bank must be checked and adjusted as necessary by a GT-R certified NISSAN dealer.