1.CHECK TRUNK LID OPENER CANCEL SWITCH Check trunk lid opener cancel switch position. Does trunk lid opener cancel switch turn OFF (CANCEL)? YES>>Turn on trunk lid opener cancel switch. NO>>GO TO 2.
2.CHECK FUNCTION

1. Use CONSULT-III to perform Active Test (“TRUNK/GLASS HATCH”).
2. Touch “OPEN” to check that it works normally.

Is the inspection result normal?
YES>>Trunk lid opener actuator is OK.
NO>>Refer to Diagnosis Procedure.