1.CHECK DOOR LOCK FUNCTION Check door lock function. Does door lock/unlock using door request switch? YES>>GO TO 2. NO-1>>Driver side: Refer to Diagnosis Procedure.
NO-2>>Passenger side: Refer to Diagnosis Procedure.
2.CHECK INTELLIGENT KEY WARNING BUZZER
Check Intelligent Key warning buzzer.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 3.
NO>>Repair or replace the malfunctioning parts.
3.CONFIRM THE OPERATION
Confirm the operation again.
Is the result normal?
YES>>Check intermittent incident. Refer to Intermittent Incident.
NO>>GO TO 1.