Use the chart below to find the cause of the symptom. If necessary, repair or replace these parts.

Reference | Inspection (GT-R certified NISSAN dealer) | — | — | — | Inspection (GT-R certified NISSAN dealer) | Inspection (GT-R certified NISSAN dealer) | Inspection (GT-R certified NISSAN dealer) | NVH in DLN section. | NVH in FAX, RAX, FSU and RSU section. | NVH in WT section. | NVH in WT section. | NVH in FAX and RAX section. | NVH in BR section. | NVH in ST section.
Possible cause and SUSPECTED PARTS | Uneven rotating torque | Center bearing improper installation | Excessive center bearing axial end play | Center bearing mounting (insulator) cracks, damage or deterioration | Excessive joint angle | Rotation imbalance | Excessive runout | DIFFERENTIAL | AXLE AND SUSPENSION | TIRE | ROAD WHEEL | DRIVE SHAFT | BRAKE | STEERING
Symptom | Noise | × | × | × | × | × | × | × | × | × | × | × | × | × | ×
Shake |  | × |  |  | × |  |  |  | × | × | × | × | × | ×
Vibration | × | × | × | × | × | × | × |  | × | × |  | × |  | ×
×: Applicable