- A high-vacuum aluminum die-casting integral molding strut housing is adopted to improve body rigidity, weight reduction, collision safety, and high accuracy.
- A high-vacuum die-casting integral molding door inner is adopted to improve glass raising/lowering performance during high-speed driving, to improve weight reduction, collision safety, high accuracy, and to improve open/close operability and closing noise.
- A high-vacuum aluminum die-casting integral molding rear seatback panel is adopted to improve body rigidity and weight reduction.

1. | Strut housing | 2. | Rear seatback support | 3. | Door inner