REMOVAL

1.Remove headlining assembly (rear) to secure work space between vehicle and headlining. Refer to Removal and Installation.

2.Remove nuts, and then remove satellite radio antenna from roof panel.

INSTALLATION
Install in the reverse order of removal.
■ CAUTION ■
Be careful about tightening torque. Antenna sensitivity becomes poor, and when it is excessive, roof panel may be deformed, when satellite radio antenna mounting nut tightening torque is loose.