1.CHECK REMOTE KEYLESS ENTRY FUNCTION Check remote keyless entry function. Does door lock/unlock with Intelligent key button? YES>>GO TO 2. NO>>Go to System Description.
2.CHECK VEHICLE SECURITY ALARM OPERATION
Check vehicle security alarm operation.
Does alarm (headlamp and horn) active?
YES>>GO TO 3.
NO>>Go to System Description.
3.CHECK “PANIC ALARM SET” SETTING IN “WORK SUPPORT”
Check “PANIC ALARM SET” setting in “WORK SUPPORT”.
Refer to CONSULT-III Function (BCM - INTELLIGENT KEY).
Is the inspection result normal?
YES>>GO TO 4.
NO>>Set “PANIC ALARM SET” setting in “WORK SUPPORT”.
4.CONFIRM THE OPERATION
Confirm the operation again.
Is the result normal?
YES>>Check intermittent incident. Refer to Intermittent Incident.
NO>>GO TO 1.