1.PERFORM E-SUS CONTROL UNIT REPROGRAMMING With CONSULT-III Reprogram “E-SUS”. Is it been completed successfully? YES>>GO TO 2.
NO >>GO TO 3.
2.PERFORM SELF-DIAGNOSIS
With CONSULT-III
Perform “E-SUS” self-diagnosis.
Is DTC “C1D23” detected?
YES>>GO TO 3.
NO>>INSPECTION END
3.PERFORM E-SUS CONTROL UNIT REPROGRAMMING AGAIN
With CONSULT-III

1. Reprogram “E-SUS”.
2. Perform “E-SUS” self-diagnosis.

Is DTC “C1D23” detected?
YES>>Replace E-SUS control unit. Refer to Exploded View (GT-R certified NISSAN dealer).
NO>>GO TO 4.
4.ERASE ERROR RECORD
Erase the memory of “E-SUS” self-diagnosis result (history).
>>END