1.SAVING VEHICLE SPECIFICATION ‐CONSULT‐III Configuration Perform “READ CONFIGURATION” to save or print current vehicle specification. Refer to Description. NOTE： If “READ CONFIGURATION” can not be used, use the “WRITE CONFIGURATION - Manual selection”.
>>GO TO 2.
2.REPLACE AV CONTROL UNIT
Replace AV control unit. Refer to Removal and Installation.
>>GO TO 3.
3.WRITING VEHICLE SPECIFICATION
‐CONSULT‐III Configuration
Perform “WRITE CONFIGURATION-Config file” or “WRITE CONFIGURATION-Manual selection” to write vehicle specification. Refer to Special Repair Requirement.
>>GO TO 4.
4.OPERATION CHECK
Check that the operation of the AV control unit is normal.
>>WORK END