- THE LARGE ILLUSTRATIONS are exploded views (see the following) and contain tightening torques, lubrication points, section number of the PARTS CATALOG (e.g. SEC. 440) and other information necessary to perform repairs.The illustrations should be used in reference to service matters only. When ordering parts, refer to the appropriate PARTS CATALOG.Components shown in an illustration may be identified by a circled number. When this style of illustration is used, the text description of the components will follow the illustration.

1. | Union bolt | 2. | Copper washer | 3. | Brake hose
4. | Cap | 5. | Bleed valve | 6. | Sliding pin bolt
7. | Piston seal | 8. | Piston | 9. | Piston boot
10. | Cylinder body | 11. | Sliding pin | 12. | Torque member mounting bolt
13. | Washer | 14. | Sliding pin boot | 15. | Bushing
16. | Torque member | 17. | Inner shim cover | 18. | Inner shim
19. | Inner pad | 20. | Pad retainer | 21. | Pad wear sensor
22. | Outer pad | 23. | Outer shim | 24. | Outer shim cover
| 1: PBC (Poly Butyl Cuprysil) grease or silicone-based grease |  | 2: Rubber grease |  | : Brake fluid
Refer to GI section for additional symbol definitions.

SYMBOLS