1. | BCM M118, M119, M120,M121, M122, M123 | 2. | Remote keyless entry receiver M134 | 3. | Inside key antenna (console) M146
4. | Outside key antenna (rear bumper) B60 | 5. | Inside key antenna (trunk room) B41 | 6. | Outside handle LH (request switch) D13
7. | Outside antenna (driver side) D24 | 8. | Inside key antenna (instrument center) M75 | 9. | Intelligent key warning buzzer (engine room) E62
10. | Trunk lid opener request switch B153 | 11. | Trunk lid opener cancel switch M105 | 12. | Combination meter M53
A. | Dash side lower (passenger side). | B. | Behind display unit. | C. | Back of rear console assembly.
D. | Behind rear bumper. | E. | Behind trunk front finisher. | F. | Back of door finisher.
G. | Back of cluster lid C (lower). | H. | Behind air cleaner box (RH). |  |

1. | Control device (detention switch) B20 | 2. | Key slot M60 | 3. | Trunk lid opener switch M20
4. | Key warning lamp | 5. | Trunk lid lock assembly B352 | 6. | Fuel lid lock actuator B244
7. | Driver side door lock actuator D15 | 8. | Power window main switch (door lock and unlock switch) D8 | 9. | Driver side door switch B21
10. | Horn low E81,E82 | 11. | Horn high E79,E80 | 12. | Push-button ignition switch M131
A. | View with center console assembly removed. | B. | View with trunk lid finisher removed. | C. | View with trunk side finisher removed.
D. | Behind front bumper |  |  |  |