DTC DETECTION LOGIC

DTC | Display Item | Malfunction detected condition | Possible causes
C1D01 | VEHICLE SPEED SIG |

- A malfunction is detected in the vehicle speed signal output from the ABS actuator and electric unit (control unit) to CAN communication.
- No transmission of vehicle speed signal from the ABS actuator and electric unit (control unit).

- Harness or connector (CAN communication line)
- ABS actuator and electric unit (control unit)
- E-SUS control unit

DTC REPRODUCTION PROCEDURE
1.DTC REPRODUCTION PROCEDURE
With CONSULT-III

1. Turn the ignition switch OFF to ON.
2. Perform “E-SUS” self-diagnosis.

Is DTC “C1D01” detected?
YES>>Proceed to diagnosis procedure. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END