1.CHECK BRAKE PEDAL STROKE Check brake pedal stroke. Refer to Inspection and Adjustment. Is the stroke too large? YES>>

- Bleed air from brake tube and hose. Refer to Bleeding Brake System.
- Check brake pedal, brake booster, and master cylinder for mount play, looseness, brake system fluid leakage, etc.

- Brake pedal: Refer to Exploded View.
- Brake booster: Refer to Exploded View (GT-R certified NISSAN dealer).
- Master cylinder: Refer to Exploded View (GT-R certified NISSAN dealer).

NO>>GO TO 2.
2.CHECK FUNCTION
Disconnect ABS actuator and electric unit (control unit) harness connector to deactivate ABS. Check if braking force is normal in this condition. Connect harness connector after inspection.
Is the inspection result normal?
YES>>Normal
NO>>Check brake system.