■ WARNING ■

- Be careful not to get burned, as engine oil may be hot.
- Prolonged and repeated contact with used engine oil may cause skin cancer. Try to avoid direct skin contact with used engine oil. If skin contact is made, wash thoroughly with soap or hand cleaner as soon as possible.

1.Warm up the engine, and check for engine oil leakage from engine components. Refer to Inspection.

2.Stop the engine and wait for 5 minutes.

3.Loosen oil filler cap.

4.Remove front undercover. Refer to Exploded View.

5.Remove drain plug (1) and then drain engine oil.

| : Vehicle front