REMOVAL Be careful with the following items when removing sensor. ■ CAUTION ■ Never twist sensor harness, when removing it. Pull sensors out without pulling sensor harness. INSTALLATION Be careful with the following items when installing wheel sensor. Tighten installation bolts to the specified torques. Refer to Exploded View (GT-R certified NISSAN dealer).
■ CAUTION ■

- When installing, check that there is no foreign matter such as iron chips on or in the mounting hole of the wheel sensor. Check that no foreign matter is caught in the sensor rotor. Remove any foreign matter and clean the mount.
- When installing wheel sensor, always press rubber grommets (A) in until they lock at the locations shown above in the figure. When installed, harness must not be twisted.