1. | Breather separator | 2. | Knock sensor | 3. | Rear oil seal
4. | Cylinder block | 5. | Thrust bearing | 6. | Oil jet
7. | Main bearing (upper) | 8. | Crankshaft key | 9. | Crankshaft
10. | Main bearing (lower) | 11. | O‐ring | 12. | Lower cylinder block
13. | Lower cylinder block bolt | 14. | Connecting rod bolt | 15. | Connecting rod bearing cap
16. | Connecting rod bearing | 17. | Connecting rod | 18. | Snap ring
19. | Piston pin | 20. | Piston | 21. | Oil ring
22. | Second ring | 23. | Top ring | 24. | Flywheel
25. | Reinforcement plate | 26. | Clamp | 27. | PCV hose
28. | PCV valve | 29. | Cylinder block heater (for Canada) |  |
A. | To intake manifold collector | B. | Refer to Disassembly and Assembly (GT-R certified NISSAN dealer) | C. | Apply neutral detergent on the outer edge.
| : Engine front |  |  |  |
Refer to Components for symbols in the figure.