Component | Description
Compressor | Intakes, compresses, and discharges refrigerant, to circulate refrigerant inside the refrigerant cycle.
Condenser | Cools refrigerant discharged from compressor, and transforms it to liquid refrigerant.
Liquid tank | Eliminates foreign matter in refrigerant, and stores temporarily liquid refrigerant.
Refrigerant pressure sensor | Refer to Description (GT-R certified NISSAN dealer).
Expansion valve | Transforms high‐pressure liquid refrigerant to mist form low‐pressure liquid refrigerant by drawing function.
Evaporator | The mist form liquid refrigerant transforms to gas by evaporation by the air conveyed from the blower motor. The air is cooled by the heat by evaporation.
Blower motor | Takes in air in the vehicle or fresh outside air, provides it forcedly to the air conditioner, and conveys it inside the vehicle.