INSPECTION AFTER INSTALLATION

- Check accelerator pedal moves smoothly within the whole operation range when it is fully depressed and released.
- Check accelerator pedal securely returns to the fully released position.
- For the electrical inspection of accelerator pedal position sensor, refer to Description (GT-R certified NISSAN dealer), Description (GT-R certified NISSAN dealer), and Description (GT-R certified NISSAN dealer).

- ■ CAUTION ■
  When harness connector of accelerator pedal position sensor is disconnected, perform “Accelerator Pedal Released Position Learning”. Refer to Description (GT-R certified NISSAN dealer).