1. | BCM M118, M119, M121, M122, M123 | 2. | IPDM E/R E4, E5, E6, E7 | 3. | TCM B45
4. | Push-button ignition switch M131 | 5. | A/T shift selector (detention switch) B20 | 6. | Key slot M60
7. | Combination meter (Key warning lamp) M53 | 8. | Driver side door switch B21 | 9. | Security indicator lamp M29
10. | Stop lamp switch E110 |  |  |  |
A. | Behind the instrument lower panel RH | B. | Engine room dash panel (RH) | C. | View with trunk front finisher removed
D. | View with center console assembly removed | E. | View with instrument lower panel (driver) removed |  |

1. | Trunk lid lock assembly (trunk room lamp switch) B352 | 2. | Remote keyless entry receiver M134 | 3. | Inside key antenna (console) M146
4. | Inside key antenna (trunk room) B41 | 5. | Inside key antenna (instrument center) M75 | 6. | Horn (high) E79, E80
7. | Horn (low) E81, E82 | 8. | Hood switch E83 | 9. | ECM M107
A. | View with trunk lid finisher removed | B. | Behind the display unit | C. | Back of the rear console assembly
D. | Behind the trunk front finisher | E. | Back of the cluster kid C (lower) | F. | Behind the front bumper
G. | Behind the instrument lower panel (assist) |  |  |  |