1.CHECK REMOTE KEYLESS ENTRY FUNCTION Check remote keyless entry function. Does door lock/unlock with Intelligent Key button? YES>>GO TO 2. NO>>Refer to System Description.
2.CHECK “LOCK/UNLOCK BY I-KEY” SETTING IN “WORK SUPPORT”
Check “LOCK/UNLOCK BY I-KEY” in “WORK SUPPORT”.
Refer to CONSULT-III Function (BCM - INTELLIGENT KEY).
Is the inspection result normal?
YES>>GO TO 3.
NO>>Set “LOCK/UNLOCK BY I-KEY” in “WORK SUPPORT”.
3.CONFIRM THE OPERATION
Confirm the operation again.
Is the result normal?
YES>>Check intermittent incident. Refer to Intermittent Incident.
NO>>GO TO 1.