1.CHECK TURN SIGNAL LAMP CONSULT-III ACTIVE TEST

1. Select "FLASHER" of BCM (FLASHER) active test item.
2. With operating the test items, check that the turn signal lamp blinks.

   LH | : Turn signal lamp LH blinking
   RH | : Turn signal lamp RH blinking
   Off | : The turn signal lamp OFF

Does the turn signal lamp blink?
YES>>Turn signal lamp circuit is normal.
NO>>Refer to Diagnosis Procedure.