DISASSEMBLY ■ CAUTION ■

- Never contact with the brake tube when the caliper is placed.
- Never hold the brake tube of caliper.
- Never subject the brake tube of caliper to impact.
- Never tighten or loosen the flare nut () of caliper unit.
- Never damage the caliper.

Remove cap and bleeder valve.
ASSEMBLY
■ CAUTION ■

- Never contact with the brake tube when the caliper is placed.
- Never hold the brake tube of caliper.
- Never subject the brake tube of caliper to impact.
- Never tighten or loosen the flare nut () of caliper unit.
- Never damage the caliper.

Install bleeder valve and cap.