DTC DETECTION LOGIC

DTC | Display Item | Malfunction detected condition | Possible causes
C1D12 | FR ACTUATOR SIG | An open or short circuit is detected in the front RH shock absorber actuator. |

- Harness or connector
- Malfunction of the front RH shock absorber actuator
- E-SUS control unit

DTC REPRODUCTION PROCEDURE
1.DTC REPRODUCTION PROCEDURE
With CONSULT-III

1. Start the engine and drive. Or perform “SHOCK ABSORBER ACTUATOR” in “ACTIVE TEST” for “E-SUS”. Refer to CONSULT-III Function (GT-R certified NISSAN dealer).
2. Perform self-diagnosis of “E-SUS”.

Is DTC “C1D12” detected?
YES>>Proceed to diagnosis procedure. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END