ABBREVIATIONS

The following abbreviations are used in this manual.

4WD | = | Four Wheel Drive Vehicles
A/C | = | Air Conditioner
A/T | = | Automatic Transmission
ABS | = | Anti-Lock Brake System
ACIS | = | Acoustic Control Induction System
ADD | = | Automatic Disconnecting Differential
CAN | = | Controller Area Network
CD | = | Compact Disc
DLC3 | = | Data Link Connector 3
ECT | = | Electronic Control Transmission
ECU | = | Electronic Control Unit
EDU | = | Electronic Driving Unit
EFI | = | Electronic Fuel Injection
EGR | = | Exhaust Gas Recirculation
ESA | = | Electronic Spark Advance
ETCS-i | = | Electronic Throttle Control System-intelligent
EVAP | = | Evaporative Emission
INT | = | Intermittent
J/B | = | Junction Block
LCD | = | Liquid Crystal Display
LH | = | Left-Hand
LHD | = | Left-Hand Drive
M/T | = | Manual Transmission
PTC | = | Positive Temperature Coefficient
R/B | = | Relay Block
RH | = | Right-Hand
RHD | = | Right-Hand Drive
SRS | = | Supplemental Restraint System
SW | = | Switch
TEMP. | = | Temperature
VRV | = | Vacuum Regulating Valve
VSV | = | Vacuum Switching Valve
VVT-i | = | Variable Valve Timing-intelligent
w/ | = | With
w/o | = | Without

*The titles given inside the components are the names of the terminals(terminal codes) and are not treated as being abbreviations.